1. What is the allowable cargo load of the LUH-72A in its normal configuration when used for MEDEVAC operations?
2. What is the primary use for the CH-47 when used during CASEVAC missions?
3. What is the crew of a LUH- 72A when not being used for MEDEVAC operations?
4. What is the total length of the high performance utility hoist?
5. When used for CASEVAC operations, what is the (ACL) for the CH-47?
6. If the obstacle on the approach route is eight meters tall and the obstacle on the departure route is ten meters tall of your PZ/LZ, what is the unusable space for the departure route?
7. What reference material covers LZ/PZ operations?
8. What are the dimensions of the reference lights that mark an additional touchdown point for cargo aircraft?
9. What is the first step in HLZ setup (LZ/PZ Operations)?
10. What size landing point is required for a CH-47 with a long line sling load during nighttime operations?
11. Why must your sleeves be rolled down when working around aircraft?
12. What reference material covers Aircraft Safety?
13. In the acronym DROP, what does the R stand for?
14. What are the three portions of the aircraft that you must avoid at all times?
15. In case of a fire, when should you exit the aircraft?
16. Define an Air Assault Operation?
17. What is a chalk/load defined as?
18. What are the six factors that determine abort criteria? 
19. What are the components of an Air Route?
20. What are the three terrain flight modes? 
21. What reference material covers Aircraft Orientation?
22. What is the cruise speed of the AH-6J/MH-6J?
23. What reference material covers Aircraft Orientation?
24. What is the maximum speed of the AH- 64?
25. What is the maximum allowable cargo load (ACL) for the MV-22 without seats?
26. What is the proper angle to approach the LUH-72A with engines running?
27. What is the crash position of the LUH-72A? 
28. How far will you move away from the aircraft after crashing?
29. What is the average gallons per hour for the AH-64?
30. What reference material covers aircraft safety?
31. What are the four basic AEROMEDEVAC missions / capabilities?
32. How many emergency exits are on a CH-47?
33. The UH-60 comes equipped with how many first aid kits?
34. How many fire extinguishers are on the UH-60?
35. What reference material covers Aeromedical Evacuation?
36. What is the allowable cargo load (ACL) for combat equipped troops for the CH-46E?
37. What is the flight time of the AH-64?
38. What is the cruising speed of the UH-60?
39. What is the maximum speed of the CH-47?
40. What are the missions of the LUH-72A?
41. Which flying/landing formation is most secure?
42. The inverted Y consists of four lights, what are they called?
43. What are the three phases of LZ/PZ operations? 
44. When utilizing the NATO T, how many lights are used to mark the touchdown point? 
45. What was the first Army MEDEVAC helicopter? 
46. What are the five stages of the reverse planning sequence?
47. What aircraft is known as the angel of mercy?
48. What is the lowest level that can coordinate an Air Assault operation?
49. What three items must be on a Soldier when working in and around rotary wing aircraft? 
50. What is the primary use of the Kendrick’s Extrication device?
51. How many phases are there for PZ/LZ Operations?
52. What two categories of factors should you take into consideration when setting up a PZ/LZ?
53. What is the fifth technical consideration factor for the selection phase?
54. What size TDP is suitable for the MV-22?
55. When dealing with obstacles, what are the four R's?
56. The ________ formation is the least secure flying and landing formation.
57. The ________ is a wind direction within 45 degrees left or right of a land heading. 
58. The NATO T will be utilized if the A/C is approaching from _____ ft above ground level (AGL) or higher. 
59. Whenever atmospheric conditions increase, the A/C capabilities will be decreased and the ___ will be reduced.
60. You should never use ______ and ______ chem lights when marking a LZ/PZ.
61. True or False? All A/C can land if the ground slope is between 8 and 15 degrees.
62. True or False? Establish Control facilities is the third step when establishing a HLZ?
63. True or False? You must use the 10:1 obstacle ratio for the left/right sides of your PZ/LZ.
64. True or False? The clock method is always from the signal person perspective?
65. True or False? If prevailing winds are 10 knots or less the A/C can land into a crosswind.
66. Name two of the four information systems.
67. What is a mission of the AH-64?
68. What is a bump plan?
69. What is the primary use of the Sked Rescue System?
70. What is a mission of the AH-6J/ MH-6J?
71. What is the flight time for the CH-47 D/F Chinook?
72. True or False? The primary missions for the UH-60 A/L/M is Air Assault & Air Movement and Casualty Evacuation.
73. What is the allowable cargo load (combat equipped troops) for the UH-60 A/L/M without seats?
74. True or False? Air Assault units are the only units that are capable of executing an Air Assault Operation.
75. A __________ is defined as personnel and equipment designated to be moved by a specific aircraft.
76. Define Command and Control.
77. In a water landing, when would you exit the aircraft?
78. What three factors affects the aircrafts capabilities?
79. What does ACP stand for in reference to Air Routes?
80. True or False? Assault Forces must be prepared for presence of opposition only on the objective.
81. What is the air transport of units, personnel, supplies, and equipment including air drops and air landing while utilizing cargo rotary wing aircraft?
82. What is an evacuation performed by dedicated, standardized medical evacuation platforms, with medical professionals who provide the timely, efficient movement and enroot care of the wounded, injured, or ill persons from the battlefield and/or other locations to MTFs.
83. How many emergency exits are on the LUH-72A?
84. True or False. The AH-64E Apache primary mission is casualty evacuation.
85. Who is the first recipient of the Air Assault Badge?
86. True or False. The crew of the CH-53 is 5 PAX?
87. True or False. Line 3 in the AEROMEDEVAC covers number of patients by type?
88. What are three portions of a rotary wing aircraft that you must avoid at all times?
89. A _________ is a location where you can maintain communication with the aircraft, have total overview of the LZ/PZ, and are able to see the entirety of the LZ/PZ. 
90. True or False. The allowable cargo load for the basic rigged litter is 400lbs.
91. What are the five stages of the reverse planning sequence?
92. What is the average gallon per hour for an unarmed OH-58?
93. Air Routes are commonly marked with ______________.
94. What is the proper angle to approach the UH-60?
95. True or False? You must roll your sleeve down when working around rotary wing aircraft for uniformity and protection, added stability and protection from the rotor blade and static electricity.
96. True or False? An armed escort is required for the CH- 47 during MASCAL.
97. How many fire extinguishers are on the LUH-72A?
98. True or False? There are 11 NATO approved flying/landing formations.
99. Which CAB has more robust fire power capability?
100. What does ROZ stand for?